Graphtec Cutting Plotter Driver OPS662 Ver.4.00
for Microsoft Windows 8.1 x64 Edition / Windows 10 x64 Edition

Thank you for choosing the Graphtec OPS662 Cutting Plotter Driver. 

The README.TXT file in each directory contains instructions on installation and
operation as well as other notes. Be sure to read them carefully before 
installing or using this driver.

Before you begin installation, check that the program disk contains the 
following:
      GDSETUP64.EXE
      GDSETUP.INI

      WIN_X64\DISK1            For Windows 8.1 x64 Edition /
      WIN_X64\GPCUT64.DLL          Windows 10 x64 Edition
      WIN_X64\GPCUTUI64.DLL
      WIN_X64\GPCUTUI.CHM
      WIN_X64\GPCUTMON64.DLL
      WIN_X64\GPCUT64.INF
      WIN_X64\GPCUT64.CAT
      WIN_X64\README.TXT
      WIN_X64\CE5000.GPD
      WIN_X64\FC2250.GPD
      WIN_X64\FC8000.GPD
      WIN_X64\FC4500.GPD
      WIN_X64\CE6000.GPD
      WIN_X64\FC8600.GPD
      WIN_X64\FCX2000.GPD
      WIN_X64\CE6000Plus.GPD
      WIN_X64\FCX4000.GPD
      WIN_X64\CE_LITE.GPD
      WIN_X64\FC9000.GPD
      WIN_X64\CE7000.GPD


Required PC specifications
(The specification needs to be higher than recommended specification
 by using OS)
* OS           : Windows 8.1 x64 Edition
                  (Windows 8.1 / Pro / Enterprise)
                 Windows 10 x64 Edition
                  (Home / Pro / Enterprise / Education)
* CPU          : 1GHz 64-bit (x64) processor or faster
* Memory       : 1GB or larger
* Display      : 1024x768 True Color
* Mouse
* CD-ROM drive
* Network interface  : 10Base-T/100Base-TX
* USB interface      : USB2.0(Full Speed)
* Serial interface   : RS-232C
* Parallel interface : Centronics parallel interface
Note:
 The interface which can be used depends on the plotter model.
 The plotter needs to be connected with either interface.


Precautions to be observed when connecting the Graphtec Cutting Plotter 
via USB.
   * Operation with other than the included driver is not guaranteed.
   * Do not connect multiple plotters to a single computer.
   * Operation is not guaranteed if the plotter is connected to a USB hub 
     or to a USB extension board.

END
